;   Prolific PL2303G VCP / PL232X CDC Series

;   plser.INF (for / Win10_DCHU)

;   Copyright (c) 2019, Prolific Technology Inc.


[version]
signature="$CHICAGO$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%PRO%
DriverVer=03/31/2022,5.1.3.2
CatalogFile=plser.cat

; ================= Device Install section =====================

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%PRO%=PRO,NTx86,NTAMD64

[SourceDisksFiles]
plser.sys=1
plser64.sys=1

[SourceDisksNames]
1=%DISK_NAME%,

[DestinationDirs] 
DefaultDestDir  = 12

[PRO.NTx86]
%DeviceDesc01% = ComPort, USB\VID_067B&PID_23A3&REV_0805
%DeviceDesc02% = ComPort, USB\VID_067B&PID_23A3&REV_0705
%DeviceDesc03% = ComPort, USB\VID_067B&PID_23A3&REV_0605
%DeviceDesc04% = ComPort, USB\VID_067B&PID_23A3&REV_0505
%DeviceDesc05% = ComPort, USB\VID_067B&PID_23A3&REV_0405
%DeviceDesc06% = ComPort, USB\VID_067B&PID_23A3&REV_0305
%DeviceDesc07% = ComPort, USB\VID_067B&PID_23A3&REV_0105
%DeviceDesc08% = ComPort, USB\VID_067B&PID_23A3&REV_0100
%DeviceDesc09% = ComPort, USB\VID_067B&PID_23A3
%DeviceDesc10% = ComPort, USB\VID_067B&PID_23B3
%DeviceDesc11% = ComPort, USB\VID_067B&PID_23C3
%DeviceDesc12% = ComPort, USB\VID_067B&PID_23D3
%DeviceDesc13% = ComPort, USB\VID_067B&PID_23E3
%DeviceDesc14% = ComPort, USB\VID_067B&PID_23F3
%DeviceDesc15% = ComPort, USB\VID_067B&PID_2323
%DeviceDesc16% = ComPort, USB\VID_067B&PID_FFFF
%DeviceDesc17% = ComPort, USB\VID_067B&PID_2320
%DeviceDesc18% = ComPort, USB\VID_067B&PID_2321&MI_00
%DeviceDesc19% = ComPort, USB\VID_067B&PID_2322

[PRO.NTAMD64]
%DeviceDesc01% = ComPort, USB\VID_067B&PID_23A3&REV_0805
%DeviceDesc02% = ComPort, USB\VID_067B&PID_23A3&REV_0705
%DeviceDesc03% = ComPort, USB\VID_067B&PID_23A3&REV_0605
%DeviceDesc04% = ComPort, USB\VID_067B&PID_23A3&REV_0505
%DeviceDesc05% = ComPort, USB\VID_067B&PID_23A3&REV_0405
%DeviceDesc06% = ComPort, USB\VID_067B&PID_23A3&REV_0305
%DeviceDesc07% = ComPort, USB\VID_067B&PID_23A3&REV_0105
%DeviceDesc08% = ComPort, USB\VID_067B&PID_23A3&REV_0100
%DeviceDesc09% = ComPort, USB\VID_067B&PID_23A3
%DeviceDesc10% = ComPort, USB\VID_067B&PID_23B3
%DeviceDesc11% = ComPort, USB\VID_067B&PID_23C3
%DeviceDesc12% = ComPort, USB\VID_067B&PID_23D3
%DeviceDesc13% = ComPort, USB\VID_067B&PID_23E3
%DeviceDesc14% = ComPort, USB\VID_067B&PID_23F3
%DeviceDesc15% = ComPort, USB\VID_067B&PID_2323
%DeviceDesc16% = ComPort, USB\VID_067B&PID_FFFF
%DeviceDesc17% = ComPort, USB\VID_067B&PID_2320
%DeviceDesc18% = ComPort, USB\VID_067B&PID_2321&MI_00
%DeviceDesc19% = ComPort, USB\VID_067B&PID_2322

;[ComPort.AddReg]
;HKR,,PortSubClass,1,01

[ComPort.NTx86]
CopyFiles=ComPort.NTx86.Copy
AddReg=ComPort.NTx86.AddReg

[ComPort.NTx86.HW]
AddReg=ComPort.HW.AddReg

[ComPort.NTx86.Services]
AddService = plserx86, 0x00000002, Serial_Service_Inst.NTx86
AddService = Serenum,,Serenum_Service_Inst

[ComPort.NTx86.Copy]
plser.sys

[ComPort.NTx86.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,plser.sys
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[ComPort.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"serenum"
HKR,,"WDF","WdfDirectedPowerTransitionEnable",0x00010001,1

[ComPort.NTAMD64]
CopyFiles=ComPort.NTAMD64.Copy
AddReg=ComPort.NTAMD64.AddReg

[ComPort.NTAMD64.HW]
AddReg=ComPort.HW.AddReg

[ComPort.NTAMD64.Services]
AddService = plser, 0x00000002, Serial_Service_Inst.NTAMD64
AddService = Serenum,,Serenum_Service_Inst

[ComPort.NTAMD64.Copy]
plser64.sys

[ComPort.NTAMD64.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,plser64.sys
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Serial_Service_Inst.NTx86]
DisplayName    = %Serial.SVCDESC%                            
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\plser.sys                            
LoadOrderGroup = Base

[Serial_Service_Inst.NTAMD64]
DisplayName    = %Serial.SVCDESC%                            
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\plser64.sys                            
LoadOrderGroup = Base

[Serenum_Service_Inst]
DisplayName    = %Serenum.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\serenum.sys
LoadOrderGroup = PNP Filter

[Strings]
PRO = "Prolific"
DeviceDesc01 = "Prolific PL2303GD USB Serial COM Port"
DeviceDesc02 = "Prolific PL2303GR USB Serial COM Port"
DeviceDesc03 = "Prolific PL2303GS USB Serial COM Port"
DeviceDesc04 = "Prolific PL2303GE USB Serial COM Port"
DeviceDesc05 = "Prolific PL2303GL USB Serial COM Port"
DeviceDesc06 = "Prolific PL2303GT USB Serial COM Port"
DeviceDesc07 = "Prolific PL2303GC USB Serial COM Port"
DeviceDesc08 = "Prolific PL2303GC USB Serial COM Port"
DeviceDesc09 = "Prolific PL2303GC USB Serial COM Port"
DeviceDesc10 = "Prolific PL2303GB USB Serial COM Port"
DeviceDesc11 = "Prolific PL2303GT USB Serial COM Port"
DeviceDesc12 = "Prolific PL2303GL USB Serial COM Port"
DeviceDesc13 = "Prolific PL2303GE USB Serial COM Port"
DeviceDesc14 = "Prolific PL2303GS USB Serial COM Port"
DeviceDesc15 = "Prolific PL2303GD USB Serial COM Port"
DeviceDesc16 = "Prolific PL2303FF USB Serial COM Port"
DeviceDesc17 = "Prolific PL2320 USB CDC Serial Port"
DeviceDesc18 = "Prolific PL2321 USB CDC Serial Port"
DeviceDesc19 = "Prolific PL2322 USB CDC Serial Port"
Serial.SVCDESC  = "Prolific PLSER Serial Port WDF Driver"
Serenum.SVCDESC = "Serenum Filter Driver"
DISK_NAME = "USB-Serial Cable Diskette"